{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Sheet2","Sheet1"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"merged":[[1,0,1,8]]}
["附件"]
["河南省2024-2026年农机购置与应用补贴机具补贴额一览表（第四批）"]
["序号","大类","小类","品目","档次名称","基本配置和参数","机具类型","补贴额（元）","备注"]
[1,"耕整地机械","整地机械","镇压器","自走式镇压机","结构型式：自走式；工作幅宽≥1.7m（可调）；镇压器型式：胶镇压辊；镇压辊材质：橡胶辊；功率≥20马力；结构质量≥850kg","非通用类",3000]
[2,"耕整地机械","整地机械","镇压器","牵引式镇压机","结构型式：牵引式；工作幅宽≥1.5m","非通用类",600]
[3,"种植施肥机械","栽植机械","插秧机","4行手扶步进式水稻插秧机","手扶步进式;4行","通用类",2100,"调整补贴额"]
[4,"种植施肥机械","栽植机械","插秧机","6行及以上手扶步进式水稻插秧机","手扶步进式;6行及以上","通用类",3600,"调整补贴额"]
[5,"种植施肥机械","栽植机械","插秧机","汽油动力4-5行四轮乘坐式水稻插秧机","四轮乘坐式;4、5行;汽油动力","非通用类",5700,"调整补贴额"]
[6,"种植施肥机械","栽植机械","插秧机","柴油动力4-5行四轮乘坐式水稻插秧机","四轮乘坐式;4、5行;柴油动力","非通用类",5700,"调整补贴额"]
[7,"种植施肥机械","栽植机械","插秧机","汽油动力6-7行四轮乘坐式水稻插秧机","四轮乘坐式;6、7行;汽油动力","非通用类",13000,"调整补贴额"]
[8,"种植施肥机械","栽植机械","插秧机","柴油动力6-7行四轮乘坐式水稻插秧机","四轮乘坐式;6、7行;柴油动力","非通用类",18200,"调整补贴额"]
[9,"种植施肥机械","栽植机械","插秧机","汽油动力8行及以上四轮乘坐式水稻插秧机","四轮乘坐式;8行及以上;汽油动力","非通用类",17100,"调整补贴额"]
[10,"种植施肥机械","栽植机械","插秧机","柴油动力8行及以上四轮乘坐式水稻插秧机","四轮乘坐式;8行及以上;柴油动力","非通用类",20400,"调整补贴额"]
[11,"种植施肥机械","栽植机械","插秧机","汽油动力6-7行辅助驾驶四轮乘坐式水稻插秧机","四轮乘坐式:6、7行;汽油动力;前装辅助驾驶(系统)设备(卫星接收机板卡类型及频点:北斗信号)","非通用类",15500,"调整补贴额"]
[12,"种植施肥机械","栽植机械","插秧机","柴油动力6-7行辅助驾驶四轮乘坐式水稻插秧机","四轮乘坐式:6、7行;柴油动力;前装辅助驾驶(系统)设备(卫星接收机板卡类型及频点:北斗信号)","非通用类",20700,"调整补贴额"]
[13,"种植施肥机械","栽植机械","插秧机","汽油动力8行及以上辅助驾驶四轮乘坐式水稻插秧机","四轮乘坐式:8行及以上;汽油动力;前装辅助驾驶(系统)设备(卫星接收机板卡类型及频点:北斗信号)","非通用类",19600,"调整补贴额"]
[14,"种植施肥机械","栽植机械","插秧机","柴油动力8行及以上辅助驾驶四轮乘坐式水稻插秧机","四轮乘坐式:8行及以上;柴油动力;前装辅助驾驶(系统)设备(卫星接收机板卡类型及频点:北斗信号)","非通用类",22900,"调整补贴额"]
[15,"种植施肥机械","栽植机械","移栽机","1—2行自走式秧苗移栽机","自走式;行数1、2行","非通用类",3800]
[16,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","20-30L多旋翼植保无人驾驶航空器","20L≤药液箱额定容量<30L;多旋翼;电动、油动、油电混动;电动须配置智能电池系统,含智能电池2组及以上;具有避障系统;具有RTK的高精度卫星导航定位系统(卫星接收机板卡类型及频点:北斗信号);具有电子围栏","通用类",7900,"调整补贴额"]
[17,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","30-50L多旋翼植保无人驾驶航空器","30L≤药液箱额定容量<50L;多旋翼;电动、油动、油电混动;电动须配置智能电池系统,含智能电池2组及以上;具有避障系统;具有RTK的高精度卫星导航定位系统(卫星接收机板卡类型及频点:北斗信号);具有电子围栏","通用类",8400,"调整补贴额"]
[18,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","50L及以上多旋翼植保无人驾驶航空器","药液箱额定容量≥50L;多旋翼;电动、油动、油电混动;电动须配置智能电池系统,含智能电池2组及以上;具有避障系统;具有RTK的高精度卫星导航定位系统(卫星接收机板卡类型及频点:北斗信号);具有电子围栏","通用类",10400,"调整补贴额"]
[19,"收获机械","粮食作物收获机械","谷物联合收割机","2-4kg/s自走式窄履带水稻收割机（全喂入）","自走履带式;喂入方式:全喂入;2kg/s≤喂入量<4kg/s;履带宽度≤400mm;直行碾压率≤30%;粮箱容积≥1.0m3;卸粮方式:自动卸粮;工作幅宽≥2000mm;功率≥50马力;离地间隙≥250mm","非通用类",21000]
[20,"收获机械","粮食作物收获机械","谷物联合收割机","4kg/s及以上自走式窄履带水稻收割机（全喂入）","自走履带式;喂入方式:全喂入;喂入量≥4kg/s;履带宽度≤450mm;直行碾压率≤35%;粮箱容积≥1.5m3;卸粮方式:自动卸粮;工作幅宽≥2000mm;功率≥70马力;离地间隙≥250mm","非通用类",26800]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}